**Low Loader Tracking Trailer No3**

Low Loading No3 Tracking Trailer is towed by a  4×4  Vehicles. More Suited for Smaller Hero Cars.

The suspension is 100% air cushion and can be adjusted according to weight and ride comfort.

For crew comfort all of our Low Loaders have a weatherproof and safe crew compartment area with bench seating and safety harnesses for 6 crew members.

The Low Loader is Driven by one of our Precision Tracking Vehicle Drivers and if used as Tracking Vehicle and Low Loader Combination – 2 Man Crew is required for its operation and Rigging.

 

|  |  |
| --- | --- |
| **Standard Equipment** | **Optional Equipment** |
| Safety Harnesses | Scaffold Tube and Fittings Rig |
| Lap belts in Crew Compartment | 5K Generator |
| **Dimensions / Weights** | |
| Overall Length of Towing Vehicle and Trailer | 13m |
| Width of Low Loader | 2.55m |
| Height of Low Loader | 2.8m |
| Working Deck of Low Loader | 5.3m x 2.55m |
| Cheyenne Tracking Vehicle Length | 6.5m |
| Cheyenne Width | 2.2m |
| Cheyenne Working Deck | 2.4mx 2.2m |
| Gross Train Weight of Tow Vehicle and Trailer | 7000kg |